# EasyFlash

---

## 1、介绍

[EasyFlash](https://github.com/armink/EasyFlash)是一款开源的轻量级嵌入式Flash存储器库，主要为MCU(Micro Control Unit)提供便捷、通用的上层应用接口，使得开发者更加高效实现基于的Flash存储器常见应用开发。该库目前提供 **三大实用功能** ：

- **Env** 小型KV数据库，支持 **写平衡（磨损平衡）** 及 **掉电保护** 模式
 
让Flash变为NoSQL（非关系型数据库）模型的小型键值（Key-Value）存储数据库。在产品上，能够更加简捷的实现 **设定参数** 或 **运行日志** 等信息掉电保存功能。

- **IAP** 在线升级再也不是难事儿
 
该库封装了IAP(In-Application Programming)功能常用的接口，支持CRC32校验，同时支持Bootloader及Application的升级。

- **Log** 无需文件系统，日志可直接存储在Flash上

非常适合应用在小型的不带文件系统的产品中，方便开发人员快速定位、查找系统发生崩溃或死机的原因。同时配合[EasyLogger](https://github.com/armink/EasyLogger)(我开源的超轻量级、高性能C日志库，它提供与EasyFlash的无缝接口)一起使用，轻松实现C日志的Flash存储功能。

### 1.1、资源占用

```
最低要求： ROM: 6K bytes     RAM: 0.5K bytes + (Env大小)

Demo平台：STM32F103RET6 + RT-Thread 1.2.2 + Env(2K bytes)
实际占用： ROM: 6K bytes     RAM: 2.6K bytes
```

### 1.2、支持平台

目前已移植硬件平台有 `stm32f10x`与 `stm32f4xx` 系列的片内Flash，这个也是笔者产品使用的平台。其余平台的移植难度不大，在项目的设计之初就有考虑针对所有平台的适配性问题（64位除外），所以对所有移植接口都有做预留。移植只需修改 [`\easyflash\port\ef_port.c`](https://github.com/armink/EasyFlash/blob/master/easyflash/port/ef_port.c) 一个文件，实现里面的擦、写、读及打印功能即可。

欢迎大家 **fork and pull request**([Github](https://github.com/armink/EasyFlash)|[OSChina](http://git.oschina.net/armink/EasyFlash)|[Coding](https://coding.net/u/armink/p/EasyFlash/git)) 。如果觉得这个开源项目很赞，可以点击[项目主页](https://github.com/armink/EasyFlash) 右上角的**Star**，同时把它推荐给更多有需要的朋友。

## 2、流程

### 2.1、Env：环境变量（KV数据库）

下图为通过控制台（终端）来调用环境变量的常用接口，演示了以下过程，这些接口都支持被应用层直接调用。

- 1、创建“温度”的环境变量，名为 `temp`，并且赋值为 `123`；
- 2、保存“温度”到Flash中并重启；
- 3、检查“温度”是否被成功保存；
- 4、修改“温度”值为 `456` 并保存、重启；
- 5、检查“温度”是否被成功修改；
- 6、删除“温度”的环境变量。

![easy_flash_env](http://git.oschina.net/Armink/EasyFlash/raw/master/docs/zh/images/EnvDemo.gif)

### 2.2、IAP：在线升级

下图演示了通过控制台来进行IAP升级软件的过程，使用的是库中自带的IAP功能接口，演示采用的是串口+Ymodem协议的方式。你还也可以实现通过CAN、485、以太网等总线，来实现远程网络更新。

![easy_flash_iap](http://git.oschina.net/Armink/EasyFlash/raw/master/docs/zh/images/IapDemo.gif)

### 2.3、Log：日志存储

下图过程为通过控制台输出日志，并将输出的日志存储到Flash中。重启再读取上次保存的日志，最后清空Flash日志。

![easy_flash_log](http://git.oschina.net/Armink/EasyFlash/raw/master/docs/zh/images/LogDemo.gif)

## 3、文档

具体内容参考[`\docs\zh\`](https://github.com/armink/EasyFlash/tree/master/docs/zh)下的文件。务必保证在 **阅读文档** 后再移植使用。

## 4、许可

采用 MIT 开源协议，细节请阅读项目中的 LICENSE 文件内容。

---

## 1 Introduction

[EasyFlash](https://github.com/armink/EasyFlash) is an open source lightweight embedded flash memory library. It provide convenient application interface for MCU (Micro Control Unit). The developers can achieve more efficient and common application development based on Flash memory. The library currently provides **Three useful features** ：

- **Env(environment variables)** : A small KV database. Support **write balance mode(wear leveling)** and **power fail safeguard**.

Let Flash becomes a small NoSQL (non-relational databases) model and Key-Value stores database. You can be more simple to store **setting parameters** or **running logs** and other information which you want to power down to save.

- **IAP** : online upgrade is no longer a difficult thing.
 
The library encapsulates the IAP (In-Application Programming) feature common interface. Support CRC32 checksum. While supporting the bootloader and application upgrade.

- **Log** : The logs can store to product's flash which has no file-system.

It's very suitable for small without a file system products. The developer can easy to locate and query problem when system crashes or freezes. You can use [EasyLogger](https://github.com/armink/EasyLogger)( A super-lightweight, high-performance C log library which open source by me. It provides a seamless interface with EasyFlash) at the same time. So, it's so easy to store the logs to flash.

### 1.1 Resource consumption

```
Minimum : ROM: 6K bytes     RAM: 0.5K bytes + (Env size)

Demo    :STM32F103RET6 + RT-Thread 1.2.2 + Env(2K bytes)
Actual  : ROM: 6K bytes     RAM: 2.6K bytes
```

### 1.2 Supported platforms

Hardware platform has been ported `stm32f10x` and `stm32f4xx` series of on-chip Flash. This is my product platform. Remaining platform porting difficulty is little. The porting just modify [`\easyflash\port\ef_port.c`](https://github.com/armink/EasyFlash/blob/master/easyflash/port/ef_port.c) file. Implement erase, write, read, print feature.

Welcome everyone to **fork and pull request**([Github](https://github.com/armink/EasyFlash)|[OSChina](http://git.oschina.net/armink/EasyFlash)|[Coding](https://coding.net/u/armink/p/EasyFlash/git)). If you think this open source project is awesome. You can press the **Star** on the top right corner of [project home page](https://github.com/armink/EasyFlash), and recommend it to more friends.

## 2 Flow

### 2.1 Env(KV database)

The figure below shows an ENV's common interface be called by the console(terminal). These interfaces are supported by the application layer called.

- 1.Create temperature environment variable. It's name is `temp` and value is `123`;
- 2.Save temperature to flash and reboot;
- 3.Check the temperature has saved successfully;
- 4.Change the temperature value to `456` and save, reboot;
- 5.Check the temperature has changed successfully;
- 6.Delete temperature environment variable.

![easy_flash_env](https://raw.githubusercontent.com/armink/EasyFlash/master/docs/en/images/EnvDemo.gif)

### 2.2 IAP

The figure below shows the process of upgrade software through the console by IAP. It use this library comes with IAP function interface. Uses a serial port + Ymodem protocol mode. You can also be achieved through CAN, 485, Ethernet bus to online upgrade.

![easy_flash_iap](https://raw.githubusercontent.com/armink/EasyFlash/master/docs/en/images/IapDemo.gif)

### 2.3 Log

The following figure is the output log process through the console. The logs will save to flash at the same time. Then reboot the and read the logs from flash. At last will clean all logs which on flash.

![easy_flash_log](https://raw.githubusercontent.com/armink/EasyFlash/master/docs/en/images/LogDemo.gif)

## 3 Documents

All documents is in the [`\docs\en\`](https://github.com/armink/EasyFlash/tree/master/docs/en) folder. Please **read the documents** before port and use it.

## 4 License

Using MIT open source license, please read the project LICENSE file.